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Technical specification LBAi W GATE Double
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Tender documents:
The ultra-fast folding gate shall be reliable and robust, designed for intensive, continuous operation with a 5 m clear opening.
It shall comply with standard 13241-1 and be validated by CSTB, with installation requiring no additional safety photocells or safety edges. It shall meet the following specifications:
Technical specifications
· Custom height of 2 m
· Double: 2 x 2 leaves for a total clear opening of 5 m
· 6 mm thick steel pivot posts – 350 x 250 mm cross-section
· Anti-corrosion e-coat treatment
· Powder coating baked at 250°, with a choice of RAL colours: White 9010, Grey 7016, Green 6005, Red 3020 or Black 9005
· Aluminium leaves with 30 x 30 mm bars and variable spacing suited to the gate length, not exceeding 110 mm
· Concealed drive integrated into the pivot post, accessible through a dedicated door below the control compartment door
· Control system accessible through two doors integrated into the pivot posts, with access when the gate is open or closed.
· (exposed motors and/or separate control cabinets shall not be permitted)
Equipment
· Reversible geared motor
· Brake motor enabling the gate to be locked in the event of a power failure
· Manual release from the motor compartment
· Opening speed of 1.2 m/s
· Force limiter in the event of impact
· Contactless inductive sensors for position control
· Held in the open or closed position
· 90° opening
· Access doors fitted with anti-vandalism compression locks
· LED area lighting
· Flashing amber light with advance warning
· 500 kg electromagnetic lock
· 2 anchoring templates with anchor rods
· Lifting eyes for easy, safe positioning by installers
Integrated ONE-C control board
· Hardwired or network cable control; several communication protocols (Modbus TCP/IP, RS485)
· Centralised communication interface (LED display)
· Remote configuration and control via web server
· Variable-frequency motor control to adjust:
· Acceleration and braking ramps
· Opening and closing speeds
· SD card updates with a single program
· Plug-in terminal block
LBAi functions
· Integrated detection without ground loops or additional infrared photocells
· No detection-related civil works and reduced wiring requirements
· Recognition of 7 user categories: pedestrians, bicycles, motorcycles, cars, vans, trucks and buses
· Up to 5 configurable detection zones
· Range up to 10 m
· 170° horizontal and 70° vertical coverage
· Precise settings to limit unwanted detections
· Configurable access permissions by category
· Management of access authorisations and denials
· Customisable time schedules
· Configuration via a secure local Wi-Fi connection, independent of the site's network
· Continuous day and night operation with reliable performance in adverse weather
· Activity log available to assist diagnostics
· Simple updates via SD card
· Planned upgrades: vehicle counting and future recognition of specific vehicles
Options to include in the tender documents if selected
· 115° opening
· Alternative colour to be selected from the RAL chart
· Perforated aluminium infill panel with an LBA Design pattern
· Ø60 mm LED light mounted on the receiver post
· Controlled red/green LED strip
· Additional 500 kg electromagnetic lock
Compliance
· Compliant with standard 13241-1
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